Synthetics
drive business.
Enquire now

Mobil's Global expertise and technological advancements help your fleet perform better by achieving better fuel efficiency**, improving your engine's life hence boosting your bottom line.

## Contact us today for a
Free engine oil testing

All fields are mandatory*
Name *
Designation *
Company *
Phone Number *
Email Id *
Fleet Size *
I agree to the ExxonMobil terms and conditions and the MSLA terms and conditions.
Any information submitted in this form will be used in accordance with ExxonMobil privacy policy.
The product performance results shown are based on the experience of individual customers. Actual results can vary depending upon the type of equipment used and its maintenance, operating conditions and environment, and any prior lubricant used.
*T&C apply.

### Top sellers

Mobil Delvac 1™
ATF
I am interested
Mobil Delvac Modern™
15W-40 Super Fleet
I am interested
Mobil Delvac 1™
ESP 5W-40
I am interested

### The Delvac effect

Find out how Delvac helps your fleet accelerate profits
Find out how Delvac helps your fleet accelerate profits
Find out how Delvac helps your fleet accelerate profits
Find out how Delvac helps your fleet accelerate profits

### Mobil Delvac™ success stories

Rivigo Logistics achieved 4% fuel efficiency
and saved ₹1,07,520 per truck

Learn how

Sri Vijayakumar Roadways achieved 3%
fuel efficiency and saved ₹57,263 per bus

Learn how

Express Roadways achieved re-greasing interval of 1,20,000 kms and saved ₹9,231 per truck

Learn how

## Product categories

Every lubricant we manufacture is as unique as the engine it's made for, catering different industry and OEM standards. Our range of lubricants comply with the recommended emission standard guidelines. Every Mobil Delvac™ engine oil ensures it meets or exceeds performance to protect the engine, its cleanliness level, aid high and low temperature performance, soot dispersion and optimize drain intervals resulting in reduced oil consumption and equipment downtime.

- Engine oil
- Hydraulic oil
- Gear & Axle oil
- Transmission oil
- Greases

## Mobil Delvac 1™ ESP 5W-40

Mobil Delvac 1™ ESP 5W-40 is an advanced synthetic heavy duty diesel engine oil that helps extend engine life while providing long drain capability and potential fuel economy for modern and latest diesel engine technology operating in severe applications. This product is formulated to deliver exceptional performance in modern and older, hard working, engines, including those with emission control systems. Mobil Delvac 1 ESP 5W-40 is recommended for use in a wide range of heavy-duty applications and operating environments found in the on-road transport and off-road mining, forestry, construction, and agricultural industries.

#### Key benefits

- Reliable engine start and wear protection at low temperatures
- Reduced engine wear to promote long engine life
- Long oil drain intervals and prevention of deposits
- Protection of critical engine surfaces in humid environments

Technical specifications I am interested

## Mobil Delvac MX™ ESP 15W-40

Mobil Delvac MX™ ESP 15W-40 is an extra high performance diesel engine oil that helps extend engine life in severe on and off-highway applications while delivering outstanding performance in modern, high-output, low-emission engines including those with Exhaust Gas Recirculation (EGR) and After treatment Systems with Diesel Particulate Filters (DPFs) and Diesel Oxidation Catalysts (DOCs). Fully backwards compatible, Mobil Delvac MX ESP 15W-40 will also deliver the same exceptional performance in older conventional engines. As a result, it meets or exceeds the requirements of the API CK-4, CJ-4, CI-4 PLUS and CH-4 service categories as well as key Original Equipment Manufacturer (OEM) requirements.

#### Key benefits

- Helps to maintain engine efficiency, long engine life and long oil life
- Helps to reduce low temperature sludge build-up and high temperature deposits
- Helps to lower oil costs due to less make-up oil during operation
- Superior soot-viscosity control
- Long gasket, seal, and after treatment (DPF and DOC) life

Technical specifications I am interested

## Mobil Delvac™ Super 15W-40

Mobil Delvac™ Super 15W-40 is high performance, heavy duty engine oils that provide complete protection to diesel engines operating in severe on and off-highway service applications. Mobil Delvac Super 15W-40 is recommended for use in a wide range of heavy duty applications and operating environments found in the trucking, construction and agricultural industries.

#### Key benefits

- Sludge build-up and deposit control
- Cleaner engines and longer engine life
- Reduced oil consumption and wear

Technical specifications I am interested

## Mobil Delvac Modern™ 15W-40 Super Fleet

Mobil Delvac Modern™ 15W-40 Super Fleet is an extra high performance synthetic technology diesel engine oil that provides excellent lubrication to both on highway and off highway diesel engines. It offers upto 60%* more wear protection than API CI-4 PLUS standards thus reducing engine mainteance cost along with long oil drain interval.
* Based on Cummins M11 EGR/Cummins ISM engine test

#### Key benefits

- Exceptional viscosity control and better engine performance
- Deposit control and acid neutralization
- Start-up wear protection
- Longer gasket and seal life

Technical specifications I am interested

## Mobil™ Hydraulic AW Series

Mobil™ Hydraulic AW Series oils are good quality anti-wear hydraulic oils intended for industrial and mobile service applications, subjected to moderate operating conditions and requiring anti-wear lubricants. They are formulated to deliver good performance in a range of hydraulic components used in systems subjected to moderate operating conditions.

#### Key benefits

- Good anti-wear performance helps reduce pump wear and prolonging pump life
- Corrosion protection helps reduce the effects of moisture on system components
- Filterability to prevent filter blockage even in the presence of water

Technical specifications I am interested

## Nuto H Series

Nuto™ H Series oils are good quality anti-wear hydraulic oils intended for industrial and mobile service applications, subjected to moderate operating conditions and requiring anti-wear lubricants. Their effective oxidation resistance and chemical stability support good oil life in moderate to severe applications.

#### Key benefits

- Good anti-wear performance helps reduce pump wear and prolonging pump life
- Corrosion protection helps reduce the effects of moisture on system components
- Filterability to prevent filter blockage even in the presence of water

Technical specifications I am interested

## Axle Oil (GL-5)

Mobilube HD™ 85W-140 is a high performance, heavy duty gear lubricant formulated from high performance base oils and an advanced additive system. This lubricant is engineered for automotive applications including heavy duty axles and final drives where extreme pressures and shock loading are expected. This is recommended by ExxonMobil for applications where API GL-5 service is required.

#### Key benefits

- Outstanding low speed/high torque wear and high speed scoring protection
- Increased load carrying capability
- Reduced maintenance costs and longer equipment life
- Minimum leakage and reduced contamination

Technical specifications I am interested

## Gear and Axle Oil (GL-4)

Mobilube GX™ 80W-90 is a high performance, heavy duty gear lubricant formulated from high quality base oils and an advanced additive system. This lubricant is engineered for automotive heavy-duty transmissions, axles, and final drives where protection against wear and scoring is required. This is recommended by ExxonMobil for use in applications where API GL-4 service is required.

#### Key benefits

- Good thermal stability
- Outstanding high temperature oxidation resistance
- Extended gear and bearing life
- Longer seal life
- Reduced wear at start-up and ease of start-up

Technical specifications I am interested

## Gear and Axle Oil

Mobilube 1™ SHC 75W-90 is a fully synthetic, high performance commercial gear lubricant formulated using advanced base oils and the latest technology additive system. This lubricant is engineered for heavy duty manual transmissions and rear axles where operations require gear lubricants with excellent load-carrying capability over wide operating temperatures and where extreme pressures and shock loading are expected. Mobilube 1 SHC 75W-90 has excellent thermal and oxidation stability, high inherent Viscosity Index (VI), extremely low pour point, and outstanding low temperature fluidity.

#### Key benefits

- Increased load-carrying capability.
- Reduced maintenance costs and long equipment life
- Retains viscosity and film strength under severe operating conditions to prevent wear
- One lubricant for heavy-duty manual transmissions and rear axles
- Minimum leakage and reduced contamination
- Fuel economy potential and improved shiftability

Technical specifications I am interested

## Mobil Delvac 1™ ATF

Mobil Delvac 1™ ATF is a fully synthetic fluid recommended by Allison Transmission, Inc. approved against the Allison TES-295 Specification. The fluid is designed to meet the demanding requirements of modern heavy duty automatic transmissions. The synthetic base oil composition enables excellent performance even in some of the harshest of operating conditions. It offers outstanding gear shifting and power transfer performance. Versus conventional ATF fluids, the inherently high viscosity index and stability of Mobil Delvac 1 ATF protects against thermal breakdown at high operating temperatures, while still providing outstanding performance at sub-zero temperatures.

#### Key benefits

- Keeps transmissions clean to extend life and performance even under some of the harshest driving conditions.
- Extended transmission life
- Provides prompt and reliable lubrication at sub-zero ambient temperatures down to –54º C.

Technical specifications I am interested

## Mobil ATF™ 220

Mobil ATF™ 220 is a high performance, fluid for automatic transmissions in older vehicles specifying Dexron IID. It is also used as a hydraulic fluid in unique applications. Mobil ATF 220 is formulated from high-quality conventional base oils combined with a special additive system including viscosity index improvers, antioxidants, and defoaments providing smooth and controlled friction/wear characteristics.

#### Key benefits

- Resists lacquer, sludge and deposit formation to keeps transmissions clean for efficient operation over the fill life.
- Assist in improved start-up and clean fast lubrication at low ambient temperatures.
- Smooth and lasting shift feel and reduced fluid loss in severe service operating conditions
- Meets the wear requirement to promote longer transmission life
- Maintains effective leakage control

Technical specifications I am interested

## Mobil Delvac™ Long Life Grease NLGI 3 grade

Mobil Delvac™ Long life Grease is a high quality, multipurpose, NLGI 3 grade, lithium grease based on an ISO VG 160 mineral oil. It is formulated to provide added protection against rusting and water washout in general purpose automotive applications at moderate temperatures and loads.

#### Key benefits

- Excellent structural stability
- Extended re-lubrication intervals
- Lead, chlorine and nitrite free
- Good resistance to water washout
- Extra protection against rust and corrosion

Technical specifications I am interested

## Mobilgrease XHP™ 222 NLGI 2 grade

Mobilgrease XHP™ 222 is recommended by ExxonMobil for industrial and marine applications, chassis components and farm equipment. Its sticky formulation stays in applications longer. These greases were designed to outperform conventional products by applying cutting edge, proprietary, lithium complex manufacturing technology. They are formulated to provide excellent high temperature performance with superb adhesion, structural stability and resistance to water contamination. These greases have a high level of chemical stability and offer excellent protection against rust and corrosion.

#### Key benefits

- Proprietary, lithium complex manufacturing technology
- Superb water washout and spray-off resistance
- Highly adhesive and cohesive structure
- Extended re-lubrication intervals
- Lowered maintenance costs

Technical specifications I am interested

### The History of Mobil Delvac™

A lot of things have changed since 1925, when Mobil Delvac™ became one of the world’s first diesel engine oils. Read on to know more about the history behind Mobil Delvac™

Know more
**T&C apply.
Mobil Mobil India mobil.b2b@exxonmobil.com
#FarakLaakarDekhiye
X

## Contact us today!

All fields are mandatory*
Name *
Designation *
Company *
Phone Number *
Email Id *
Fleet Size *
I agree to the ExxonMobil terms and conditions and the MSLA terms and conditions.
Any information submitted in this form will be used in accordance with ExxonMobil privacy policy.
The product performance results shown are based on the experience of individual customers. Actual results can vary depending upon the type of equipment used and its maintenance, operating conditions and environment, and any prior lubricant used.

Mobil Delvac 1™ ESP 5W-40

Property

Grade | SAE 5W-40
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 84
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 13.8
Cold-Cranking Simulator, Apparent Viscosity @ -30 C, mPa.s, ASTM D5293 | 6510
Mini-Rotary Viscometer, Apparent Viscosity, -35 C, mPa.s, ASTM D4684 | 16800
Hi-Temp Hi-Shear Viscosity @ 150 C 1x10(6) sec(-1), mPa.s, ASTM D4683 | 3.8
Viscosity Index, ASTM D2270 | 150
Ash, Sulfated, mass%, ASTM D874 | 1
Total Base Number, mgKOH/g, ASTM D2896 | 12
Pour Point, °C, ASTM D97 | -48
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 233
Density, 15.6C, g/cm3, ASTM D4052 | 0.852

Mobil Delvac MX™ ESP 15W-40

Property

Grade | SAE 15W-40
Density @ 15 C, g/ml, ASTM D1298 | 0.875
Ash, Sulfated, mass%, ASTM D874 | 0.9
Viscosity Index, ASTM D2270 | 130
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 225
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 109
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 14
Total Base Number, mgKOH/g, ASTM D4739 | 9
Pour Point, °C, ASTM D97 | -33

Mobil Delvac™ Super 15W-40

Property

Grade | SAE 15W-40
Density @ 15 C, g/ml, ASTM D1298 | 0.874
Total Base Number, mgKOH/g, ASTM D2896 | 6
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 15
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 117
Ash, Sulfated, mass%, ASTM D874 | 0.7
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 234
Pour Point, °C, ASTM D97 | -27

Mobil Delvac Modern™
15W-40 Super Fleet

Property

Grade | SAE 15W-40
Viscosity Index, ASTM D2270 | 137
Total Base Number, mgKOH/g, ASTM D2896 | 11
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 109
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 14.5
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 226
Density @ 15 C, g/cm3, ASTM D1298 | 0.877
Ash, Sulfated, mass%, ASTM D874 | 1.4

Mobil™ Hydraulic AW Series

Property

Grade | ISO 46 | ISO 68 | ISO 100
Density @ 15 C, kg/l, ASTM D4052 | 0.877 | 0.88 | 0.885
FZG Scuffing, Fail Stage, DIN 51354 | 10 | 10 | 10
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 228 | 238 | 252
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 6.9 | 8.8 | 11.2
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 46.1 | 67.9 | 99.7
Pour Point, °C, ASTM D97 | -15 | -12 | -9
Viscosity Index, ASTM D2270 | 104 | 101 | 98

Nuto H Series

Property

Grade | ISO 32 | ISO 46 | ISO 68 | ISO 100
Copper Strip Corrosion, 3 h, 100 C, Rating, ASTM D130 | 1A | 1A | 1A | 1A
Density @ 15 C, kg/l, ASTM D1298 | 0.872 | 0.876 | 0.882 | 0.884
Emulsion, Time to 3 mL Emulsion, 54 C, min, ASTM D1401 | 15 | 15 | 20 |
Emulsion, Time to 3 mL Emulsion, 82 C, min, ASTM D1401 |  |  |  | 10
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 212 | 226 | 234 | 242
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 5.3 | 6.6 | 8.3 | 11
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 31.4 | 44 | 63.3 | 96
Pour Point, °C, ASTM D97 | -24 | -24 | -18 | -18
Viscosity Index, ASTM D2270 | 98 | 98 | 98 | 98

Mobilube HD 85W-140

Property

SAE Grade | 85W-140
Viscosity, ASTM D 445 |
cSt @ 40ºC | 328
cSt @ 100ºC | 25.3
Viscosity Index, ASTM D 2270 | 97
Pour Point, ºC, ASTM D 97 | -18
Flash Point, ºC, ASTM D 92 | 224
Density @ 15ºC kg/l, ASTM D 4052 | 0.91

Mobilube GX 80W-90

Property

Grade | SAE 80W-90
Density @ 15.6 C, g/ml, ASTM D4052 | 0.89
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 240
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 14.5
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 135
Pour Point, °C, ASTM D97 | -33
Viscosity Index, ASTM D2270 | 104

Mobilube™ 1 SHC 75W-90

Property

SAE Grade | 75W-90
Viscosity, ASTM D 445 |
cSt @ 40ºC | 102
cSt @ 100ºC | 15.1
Viscosity Index, ASTM D 2270 | 156
Pour Point, ºC, ASTM D 97 | -54
Flash Point, ºC, ASTM D 92 | 202
Density @ 15ºC kg/l, ASTM D 4052 | 0.87

Mobil Delvac 1™ ATF

Property

Brookfield Viscosity @ -40 C, mPa.s, ASTM D2983 | 8400
Color, AMS 1771 | Red
Density @ 15.6 C, g/ml, ASTM D4052 | 0.85
Flash Point, °C, ASTM D92 | 236
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 7.3
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 39
Pour Point, °C, ASTM D97 | -54
Viscosity Index, ASTM D2270 | 168

Mobil ATF™ 220

Property

Brookfield Viscosity @ -40 C, mPa.s, ASTM D2983 | 33000
Color, Visual | Red
Density @ 15 C, g/ml, ASTM D4052 | 0.87
Flash Point, Cleveland Open Cup, °C, ASTM D92 | 200
Kinematic Viscosity @ 100 C, mm2/s, ASTM D445 | 7
Kinematic Viscosity @ 40 C, mm2/s, ASTM D445 | 37
Pour Point, °C, ASTM D97 | -44
Viscosity Index, ASTM D2270 | 153

Mobil Delvac™ Long Life Grease

Property

NLGI |  |  | Grade 3
Soap Type |  |  | Lithium
Color | Visual |  | Red
Structure | Visual |  | Smooth
Penetration, Worked | ASTM D217 | 0.1 mm | 235
Dropping Point | ASTM D2265 | Deg C | 180
Viscosity of Oil @ 40 Deg C | ASTM D445 | cSt | 160

Mobilgrease XHP™ 222
NLGI 2 grade

Property

Grade | NLGI 2
Thickener Type | Lithium Complex
Base Oil Viscosity of Greases @ 40 C, mm2/s, AMS 1697 | 220
Bomb Oxidation, Pressure Drop, 100 h, kPa, ASTM D942 | 35
Color, Visual | Dark blue
Copper Strip Corrosion, Rating, ASTM D4048 | 1B
Corrosion Preventive Properties, Rating, ASTM D1743 | PASS
Dropping Point, °C, ASTM D2265 | 290
Four-Ball Extreme Pressure Test, Weld Load, kgf, ASTM D2596 | 315
Four-Ball Wear Test, Scar Diameter, mm, ASTM D2266 | 0.5
Penetration, 60X, 0.1 mm, ASTM D217 | 280
Roll Stability, Penetration Consistency Change, 0.1 mm, ASTM D1831 | 0
SKF Emcor Rust Test, Distilled Water, ASTM D6138 | 0,0
Timken OK Load, kg, ASTM D2509 | 40